SCANLAB HPGL Converter Software Readme

***************************************************************************

The HPGL conversion program HPGL.EXE is supplied for testing the control
of scan systems via an RTC3 board. This program lets you load graphics
files in Hewlett Packard’s HPGL format for transfer to the RTC3 board.

***************************************************************************

Manufacturer
        SCANLAB AG
        Siemensstr. 2a
        82178 Puchheim
        Germany

        Tel.    + 49 (89) 800 746-0
        Fax:    + 49 (89) 800 746-199

        info@scanlab.de
        www.scanlab.de

***************************************************************************

How to use:

- Copy the HPGL converter and the supplied demo file into the same
  directory as the driver DLL, the RTC3 DSP program file(s) and
  correction file(s).

- Start the HPGL converter.

- Under Options|Correction select a correction file and
  under File|HPGL-File select a plot file (Demofile).

- Start output via Mark|Start Marking.